Raspberry Pi Critical Infrastructure Simulation Notes

* The Raspberry Pi’s network settings must be configured to whichever network you plan to run it off of prior to starting
* The username is ‘pi’ and the password is ‘password’ Clever, I know
* The webserver can be started by navigating to ‘/home/pi/Website’ on the pi and running the command ‘node server.js’ You can do this through SSH if you have the network set up or through a keyboard and a monitor
* To connect to the website, find the Pi’s IP and connect to it, there are 3 buttons that correspond to GPIO pins that feed into the relay